//+------------------------------------------------------------------+
//|                                           DoubleCCI-With_EMA.mq4 |
//|                   Copyright © 2005, Jason Robinson (jnrtrading). |
//|                                      http://www.jnrtrading.co.uk |
//+------------------------------------------------------------------+
//mod kino ff http://www.forexfactory.com/showthread.php?t=71075&page=6

#property copyright "Copyright © 2005, Jason Robinson (jnrtrading)."
#property link      "http://www.jnrtrading.co.uk"

#property indicator_separate_window
#property indicator_buffers 8
#property indicator_color1 DarkGreen
#property indicator_color2 Maroon
#property indicator_color3 Lime
#property indicator_color4 Red
#property indicator_color5 OliveDrab
#property indicator_color6 Lavender
#property indicator_color7 Yellow
#property indicator_color8 Blue

#property indicator_width1 4
#property indicator_width2 4
#property indicator_width3 4
#property indicator_width4 4
#property indicator_width5 3   
#property indicator_width5 3
#property indicator_width6 2
#property indicator_width7 2 


#property indicator_level1 100
#property indicator_level2 250
#property indicator_level3 350
#property indicator_level4 -350
#property indicator_level5 -250
#property indicator_level6 -100
//#property indicator_level7 0

#property indicator_levelcolor DimGray

//---- input parameters
extern int TrendCCI_period = 88;
extern int EntryCCI_period = 22;
extern bool Zero_cross_alert = true;
extern int Alert_level__Includes_negative = 100;

extern bool Show_SMA = true;
extern int SMA_period=30;

extern int periodeSMA=50;
extern int zoom=10000;


extern string SMA_of_TrendCCI_or_EntryCCI = "EntryCCI";
extern bool Automatic_timeframe_setting;
extern int M1_TrendCCI_period = 88;
extern int M1_EntryCCI_period = 22;
extern int M5_TrendCCI_period = 88;
extern int M5_EntryCCI_period = 22;
extern int M15_TrendCCI_period = 14;
extern int M15_EntryCCI_period = 6;
extern int M30_TrendCCI_period = 14;
extern int M30_EntryCCI_period = 6;
extern int H1_TrendCCI_period = 14;
extern int H1_EntryCCI_period = 6;
extern int H4_TrendCCI_period = 14;
extern int H4_EntryCCI_period = 6;
extern int D1_TrendCCI_period = 14;
extern int D1_EntryCCI_period = 6;
extern int W1_TrendCCI_period = 14;
extern int W1_EntryCCI_period = 6;
extern int MN_TrendCCI_period = 14;
extern int MN_EntryCCI_period = 6;



double TrendCCIBuffer[];
double CCIHistogramUpBuffer[];
double CCIHistogramUpUpBuffer[];
double CloseSmaBuffer[];

double CCIHistogramDownBuffer[];
double CCIHistogramDownDownBuffer[];

double EntryCCIBuffer[];
double SMA[];
//double ZeroLine[];
//+------------------------------------------------------------------+
//| Custom indicator initialization function                         |
//+------------------------------------------------------------------+
int init()
  {
//---- indicators
   SetIndexStyle (0, DRAW_HISTOGRAM, 0, 3);
   SetIndexBuffer(0, CCIHistogramUpBuffer);
   
   SetIndexStyle (1, DRAW_HISTOGRAM, 0, 3);
   SetIndexBuffer(1, CCIHistogramDownBuffer);

   SetIndexStyle (2, DRAW_HISTOGRAM, 0, 3);
   SetIndexBuffer(2, CCIHistogramUpUpBuffer);
   
   SetIndexStyle (3, DRAW_HISTOGRAM, 0, 3);
   SetIndexBuffer(3, CCIHistogramDownDownBuffer);
  
   SetIndexStyle (4, DRAW_LINE, STYLE_SOLID, 2);
   SetIndexBuffer(4, TrendCCIBuffer);


   SetIndexBuffer(5, SMA);
   SetIndexStyle (5, DRAW_LINE, STYLE_SOLID, 1);
   
   SetIndexStyle (6, DRAW_LINE, STYLE_SOLID, 2);
   SetIndexBuffer(6, EntryCCIBuffer);

        
   
   SetIndexStyle (7, DRAW_LINE, STYLE_SOLID, 1);
   SetIndexBuffer(7, CloseSmaBuffer);
   
   
   
//----
   return(0);
  }
//+------------------------------------------------------------------+
//| Custor indicator deinitialization function                       |
//+------------------------------------------------------------------+
int deinit()
  {
//---- 
   
//----
   return(0);
  }
//+------------------------------------------------------------------+
//| Custom indicator iteration function                              |
//+------------------------------------------------------------------+
int start() {

   int limit, trendCCI, entryCCI;
   static datetime prevtime = 0;
   int counted_bars = IndicatorCounted();
//---- check for possible errors
   if(counted_bars < 0) return(-1);
//---- last counted bar will be recounted
   if(counted_bars > 0) counted_bars--;

   limit=Bars-counted_bars;
   
   if (Automatic_timeframe_setting == true) 
   {
      switch(Period()) 
      {
         case 1: trendCCI = M1_TrendCCI_period; entryCCI = M1_EntryCCI_period; break;
         case 5: trendCCI = M5_TrendCCI_period; entryCCI = M5_EntryCCI_period; break;
         case 15: trendCCI = M15_TrendCCI_period; entryCCI = M15_EntryCCI_period; break;
         case 30: trendCCI = M30_TrendCCI_period; entryCCI = M30_EntryCCI_period; break;
         case 60: trendCCI = H1_TrendCCI_period; entryCCI = H1_EntryCCI_period; break;
         case 240: trendCCI = H4_TrendCCI_period; entryCCI = H4_EntryCCI_period; break;
         case 1440: trendCCI = D1_TrendCCI_period; entryCCI = D1_EntryCCI_period; break;
         case 10080: trendCCI = W1_TrendCCI_period; entryCCI = W1_EntryCCI_period; break;
         case 43200: trendCCI = MN_TrendCCI_period; entryCCI = MN_EntryCCI_period; break;
      }
   }
   else 
      {
      trendCCI = TrendCCI_period;
      entryCCI = EntryCCI_period;
      }
      IndicatorShortName("(TrendCCI: " + trendCCI + ", EntryCCI: " + entryCCI + ") ");   
      
      for(int i = 0; i <= limit; i++) 
      {
        TrendCCIBuffer[i] = iCCI(NULL, 0, trendCCI, PRICE_TYPICAL, i);
      
      if (TrendCCIBuffer[i] >= 0 && TrendCCIBuffer[i] <= 100 )
         CCIHistogramUpBuffer[i] = TrendCCIBuffer[i];
      else
         CCIHistogramUpBuffer[i] = 0;
         
      if (TrendCCIBuffer[i] >= 100 )
         CCIHistogramUpUpBuffer[i] = TrendCCIBuffer[i];
      else
         CCIHistogramUpUpBuffer[i] = 0  ; 
    
      if (TrendCCIBuffer[i] < -100 )
         CCIHistogramDownDownBuffer[i] = TrendCCIBuffer[i];
      else
         CCIHistogramDownDownBuffer[i]=0;
         
      if (TrendCCIBuffer[i] < 0  && TrendCCIBuffer[i] >=-100)
         CCIHistogramDownBuffer[i] = TrendCCIBuffer[i];
      else
         CCIHistogramDownBuffer[i]=0;   
         
      
      EntryCCIBuffer[i] = iCCI(NULL, 0, entryCCI, PRICE_TYPICAL, i);
      CloseSmaBuffer[i] =-zoom*(iMA(NULL,0,periodeSMA,0,MODE_SMA,PRICE_CLOSE,i)-Close[i]);
      //ZeroLine[i] = 0;      
      
      }

   
   
   if (Zero_cross_alert == true) {
      if (prevtime == Time[0]) {
         return(0);
      }
      else {
         if(EntryCCIBuffer[0] < -Alert_level__Includes_negative) {
            if((TrendCCIBuffer[0] < -Alert_level__Includes_negative) && (TrendCCIBuffer[1] >= -Alert_level__Includes_negative)) {
               Alert(Symbol(), " M", Period(), " Trend & Entry CCI Have both crossed below zero");
                  }
               }
     else if(EntryCCIBuffer[0] > Alert_level__Includes_negative) {
            if((TrendCCIBuffer[0] > Alert_level__Includes_negative) && (TrendCCIBuffer[1] <= Alert_level__Includes_negative)) {
               Alert(Symbol(), " M", Period(), " Trend & Entry CCI Have both crossed above zero");
                  }
               }
         prevtime = Time[0];
         }
   
     if (Show_SMA == true) 
   {
      if (SMA_of_TrendCCI_or_EntryCCI == "TrendCCI")
         for(i=0; i<limit; i++)
            SMA[i] = iMAOnArray(TrendCCIBuffer, 0, SMA_period, 0, MODE_SMA, i);
      else if (SMA_of_TrendCCI_or_EntryCCI == "EntryCCI")
         for(i=0; i<limit; i++)
            SMA[i] = iMAOnArray(EntryCCIBuffer, 0, SMA_period, 0, MODE_SMA, i);
   } 
 
 
 
 
   
   }  
   
    
//----
   return(0);
  }
//+------------------------------------------------------------------+